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Aspen Dental Management Inc.


Thursday, July 23, 2026
To All Bidders,

You are invited to bid on the new Aspen Dental office located at:

[image: image1.png]PROJECT ADDRESS

715 PROGRESS WAY
GAITHERSBURG, MD 20877




All bids are due by (5:00 PM EST) on Monday, August 24, 2026.
You will need to install the under slab plumbing and electric in September/October 2026 Framing will start in November/ December 2026. RTU’s and curbs will be supplied by TAG. 
RTU Information –DO NOT CONTACT CARRIER FOR PRICING ON THE RTU’S AND CURBS. THEY WILL BE SUPPLIED BY TAG.  YOU WILL NEED TO PRICE INSTALL ONLY. 
DARK SHELL, Landlord work is very minor and is listed below.  Please review all plans and spec’s carefully, and specifically breakout your bid as listed on our enclosed bid sheet.  
Base Building:
Base building structure and building enclosure components are complete, including exterior walls, roof, storefront and concrete floor slab. Front and rear door locations to be coordinated with Tenants floor plan.
Floor:
               Concrete slab smooth and ready for Aspen flooring. (Any imperfections in slab are to be noted and brought to Aspen’s 

attention immediately) 
Storefront:
Storefront with entry door(s) ¼” clear glass in clear anodized / bronze aluminum frame and windows insulated clear glass in 4-¼” clear anodized / bronze aluminum frame.  

Walls:
Interior and perimeter walls shall be constructed per the responsibility matrix on sheet T2.0 of the drawings.
Service Door:
One standard 36” metal rear service door.

Utilities:
All utilities to be stubbed to the Premises as shown on the plans, with the following specifications:

Electricity:  Tenant is responsible for meter and electrical feed from gutter to tenant panel.
Cable: 2” empty conduit from the building’s demarcation point to the Premises with pull string.
Telephone:  2” empty conduit from the building’s demarcation point to the Premises with pull string.

Gas:  Tenant is responsible for meter and extension of service line to the Premises.

Water:  Minimum one inch (1”) water service stubbed inside Premises and with shut of installed.

Sewer:  Four-inch (4”) sanitary sewer service stubbed inside rear of Premises and capped.  The invert elevation of the sanitary line shall be a minimum of minus 30” below finish floor.
HVAC: N/A
Required Subcontractors Include:

· Roofing Contractor
Orndorff & Spaid, Inc.
11722 Old Baltimore Pike
Beltsville, MD 20705-1292
Jason Kennedy
jason@osroofing.com
· Storefront
Skyline Construction, Inc.
14533 Sixes Road
Emmitsburg, MD 21727
Chic Wivell
cwskyline@yahoo.com
· Fire Sprinkler
Pye-Barker Fire & Safety
445 Defense Highway, Suite C
Annapolis, MD 21401
Rob Morgan
robert.morgan@pyebarkerfs.com
· Fire Alarm
Pro-Tech Electrical Contractors
7951 Gainsford Court Suite 125
Bristow, VA 20136
Nick Bryant
nbryant@pro-techsvc.com
The required documents are:

-Bid Cover sheet
- Bid Sheet
-1 set of drawings including sheets:
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If you have any questions my E-mail address is pzieno@aspendental.com. Please submit your bids via E-Mail to my attention.
Sincerely, 

Patrick D. Zieno

Patrick D. Zieno

Construction Manager
TAG – THE ASPEN GROUP
Corporate Offices      281 Sanders Creek Parkway, East Syracuse, New York 13057    Tel:  315-454-6000     Fax:  315-454-6324
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