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INSTALLATION
Install in accordance with manufacturer's instructions.
Cut and Miter Schluter-VINPRO profiles with Freud Tooth Carbide Tipped Miter Saw Blade for Non-Ferrous Aluminum Cutting Fine Finish or equal.
See proper cutting and mitering of aluminum Schluter Systems Profiles:
https://www.youtube.com/watch?v=s0kGTJp01RE
Adhere Schluter Systems VINPRO profiles to polycarbonate panels and align using Schluter-KERDI-FIX adhesive or equal.  Flat trowel the KERDI FIX to allow for flush fit to substrate.  Remove any KERDI-FIX from the exposed Schluter Profiles and polycarbonate panels using mineral spirts.
See recommend cleaning and removal of excess KERDI-FIX:
https://www.youtube.com/watch?v=7LY2q4bgEXg
Contact Earl Maicus with Schluter Systems at emaicus@schluter.com or Cel: 518-420-3618 for installation and product support. 

Earl Maicus
Senior National Accounts Manager
Schluter Systems L.P.
Cel: 518-420-3618
Email: emaicus@schluter.com
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