SCOPE INFORMATION
Advance Auto Parts #6270 - Cartersville, GA

Project: Advance Auto Parts #6270 - Cartersville, GA
Address: 914 Joe Frank Harris Parkway, Cartersville, GA 30120
Project Type: Upfit
Working Area: 24,164 SF (construction drawing gross SF)
Store Open / End Date: April 15, 2027
Construction Start: Not provided / needs updated
Landlord Scope
Hazmat remediation - verify against LOI/work letter.
Structure.
Roof in good watertight condition.
Remove existing FF&E.
Utility metering.
Parking lot as-is.
Electrical as-is.
Demolition
Remove flooring and mastic down to slab for new prototype finish throughout the first floor.
Existing storefront swing doors remain; paint black. Paint existing storefront frames black.
Existing front soffit and ACT grid remain.
Remove existing lights for new US LED layout.
Remove trim molding from column enclosures and patch drywall.
Remove existing first-floor restroom and offices for new restrooms.
Mezzanine generally remains; repair/replace toilet-room fixtures and accessories.
Remove abandoned low voltage, blocking, conduit, and similar items from perimeter walls.
Remove existing mop sink.
Modify rear sales soffit/ceiling while maintaining 13'-6" clear.
Remove and replace overhead door.
Remove rear soffit and demising wall while saving CMU office core under mezzanine.
Architectural / Finishes
New prototype slab finish in sales area.
New toilet-room bars and accessories at first floor and mezzanine.
Existing entry swing doors remain with new hardware.
Paint perimeter walls.
New US LED lighting surface-mounted to existing ACT.
Pressure wash loading ramp/platform and front walk.
New restroom finishes at new toilet rooms.
VCT in first-floor toilet rooms and main-level offices.
Remove existing ceiling pads over sales for spot replacement and provide new ceiling pads as required.
New overhead door, rear storage door, exterior rear doors and hardware.
Add edge-of-dock leveler at truck platform.
Mechanical
Replace HVAC equipment greater than 10 years old.
Remove air handler.
Review tonnage per SF; add unit or upsize RTUs as required.
Provide air curtain above entry doors.
Replace thermostats in new AAP prototype locations.
Remove abandoned rooftop equipment.
Provide new RTU sensors on conduit at 7 feet.
Existing BOH unit heaters remain.
Provide new toilet-room exhaust fans.
Plumbing
Provide new water heater.
Remove existing mop sink and provide new mop sink/faucet in old location.
Remove existing drinking fountain.
Provide new hi/lo drinking fountain at new restrooms.
Provide new fixtures at first-floor restrooms.
Replace mezzanine toilets, lavatory faucets, and urinal flush valve.
Existing exterior hose bibb at front remains.
Electrical
Provide new US LED surface-mounted lighting over existing ACT.
Existing electrical equipment remains.
Provide new LED under-canopy lights.
IT rack on first floor next to electrical.
Provide new wall packs at loading as required; re-lamp existing fixtures that remain.
Add exterior outlet at front of store.
Provide electrical requirements associated with two building sign locations.
Site / Civil
Clean existing walks.
Remove exterior cart railings.
Verify potential rails required at loading platform.
Add ramp at HUB door.
Add dock leveler at truck dock.
Signage / Exterior Facades
New front signage and side facade per SAR.
Clean and wash existing exterior.
Paint black behind sign.
Paint existing red window frames black.
Paint underside of canopy.
Two sign locations; black paint at both signs.
Fire Sprinkler / Fire Alarm
Existing sprinkler and fire alarm systems to be modified under separate permit.
Rework sprinkler heads where existing ceiling/soffit is removed or modified.
Existing riser/panel is at rear of space.
ADA
Provide new ADA accessories/grab bars in existing restroom areas as required.
Verify 2024 code changes.
Mezzanine
Existing office finishes remain as-is.
Provide new lavatory faucet.
Replace toilets.
Clean floors and walls.
Spot replace ceiling pads.
Provide new lights.
Replace urinal flush valve.
Permitting / Coordination
Building permit review noted as approximately 2-6 weeks through online portal; no expedited review.
Low-voltage permit not required per kickoff notes.
Racking permit not required per kickoff notes.
Include TELGIAN when bringing MEP engineers onto the project.




